{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["名称定義","ﾃﾞﾊﾞｲｽ展開"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"名称定義","index":0,"n_rows":36,"n_cols":3,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"軸番号","軸名称"]
[null,1,"機器１"]
[null,2,"機器２"]
[null,3,"機器３"]
[null,4,"機器４"]
[null,5,"機器５"]
[null,6,"機器６"]
[null,7,"機器７"]
[null,8,"機器８"]
[null,9,"機器９"]
[null,10,"機器１０"]
[null,11,"機器１１"]
[null,12,"機器１２"]
[null,13,"機器１３"]
[null,14,"機器１４"]
[null,15,"機器１５"]
[null,16,"機器１６"]
[null,17,"機器１７"]
[null,18,"機器１８"]
[null,19,"機器１９"]
[null,20,"機器２０"]
[null,21,"機器２１"]
[null,22,"機器２２"]
[null,23,"機器２３"]
[null,24,"機器２４"]
[null,25,"機器２５"]
[null,26,"機器２６"]
[null,27,"機器２７"]
[null,28,"機器２８"]
[null,29,"機器２９"]
[null,30,"機器３０"]
[null,31,"機器３１"]
[null,32,"機器３２"]

{"sheet":"ﾃﾞﾊﾞｲｽ展開","index":1,"n_rows":644,"n_cols":12,"rows_kept":644,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,"凡例"]
["M",{"$nulls":5},"M",null,null,null,"M"]
[2400,"位置決始動完了",null,null,1,"機器１",2400,"1軸機器１位置決始動完了",1,"機器１",3200,"1軸機器１停止指令"]
[2401,"位置決完了",null,null,1,"機器１",2401,"1軸機器１位置決完了",1,"機器１",3201,"1軸機器１急停止指令"]
[2402,"In-position",null,null,1,"機器１",2402,"1軸機器１In-position",1,"機器１",3202,"1軸機器１正転JOG指令"]
[2403,"指令In-position",null,null,1,"機器１",2403,"1軸機器１指令In-position",1,"機器１",3203,"1軸機器１逆転JOG指令"]
[2404,"速度制御中",null,null,1,"機器１",2404,"1軸機器１速度制御中",1,"機器１",3204,"1軸機器１完了信号OFF指令"]
[2405,"速度・位置Latch",null,null,1,"機器１",2405,"1軸機器１速度・位置Latch",1,"機器１",3205,"1軸機器１速度・位置切替許可"]
[2406,"零点通過",null,null,1,"機器１",2406,"1軸機器１零点通過",1,"機器１",3206,"1軸機器１位置決ﾃﾞｰﾀ更新待ち"]
[2407,"Error検出",null,null,1,"機器１",2407,"1軸機器１Error検出",1,"機器１",3207,"1軸機器１ｴﾗｰリセット"]
[2408,"ServoError検出",null,null,1,"機器１",2408,"1軸機器１ServoError検出",1,"機器１",3208,"1軸機器１ｻｰﾎﾞｴﾗｰリセット"]
[2409,"原点復帰要求",null,null,1,"機器１",2409,"1軸機器１原点復帰要求",1,"機器１",3209,"1軸機器１始動時の停止入力無効"]
[2410,"原点復帰完了",null,null,1,"機器１",2410,"1軸機器１原点復帰完了",1,"機器１",3210,"1軸機器１ﾕｰｻﾞ使用不可"]
[2411,"FLS 検出",null,null,1,"機器１",2411,"1軸機器１FLS 検出",1,"機器１",3211,"1軸機器１ﾕｰｻﾞ使用不可"]
[2412,"RLS 検出",null,null,1,"機器１",2412,"1軸機器１RLS 検出",1,"機器１",3212,"1軸機器１送り現在値更新指令"]
[2413,"STOP 検出",null,null,1,"機器１",2413,"1軸機器１STOP 検出",1,"機器１",3213,"1軸機器１ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[2414,"DOG/CHANGE 検出",null,null,1,"機器１",2414,"1軸機器１DOG/CHANGE 検出",1,"機器１",3214,"1軸機器１ｶﾑ基準位置設定指令"]
[2415,"ServoReady",null,null,1,"機器１",2415,"1軸機器１ServoReady",1,"機器１",3215,"1軸機器１ｻｰﾎﾞｵﾌ指令"]
[2416,"ﾄﾙｸ制御中",null,null,1,"機器１",2416,"1軸機器１ﾄﾙｸ制御中",1,"機器１",3216,"1軸機器１ﾕｰｻﾞ使用不可"]
[2417,"ﾕｰｻﾞ使用不可",null,null,1,"機器１",2417,"1軸機器１ﾕｰｻﾞ使用不可",1,"機器１",3217,"1軸機器１ﾕｰｻﾞ使用不可"]
[2418,"仮想ﾓｰﾄﾞ継続不可",null,null,1,"機器１",2418,"1軸機器１仮想ﾓｰﾄﾞ継続不可",1,"機器１",3218,"1軸機器１ﾕｰｻﾞ使用不可"]
[2419,"Mｺｰﾄﾞ出力中",null,null,1,"機器１",2419,"1軸機器１Mｺｰﾄﾞ出力中",1,"機器１",3219,"1軸機器１FIN信号"]
[{"$nulls":4},2,"機器２",2420,"2軸機器２位置決始動完了",2,"機器２",3220,"2軸機器２停止指令"]
[3200,"停止指令",null,null,2,"機器２",2421,"2軸機器２位置決完了",2,"機器２",3221,"2軸機器２急停止指令"]
[3201,"急停止指令",null,null,2,"機器２",2422,"2軸機器２In-position",2,"機器２",3222,"2軸機器２正転JOG指令"]
[3202,"正転JOG指令",null,null,2,"機器２",2423,"2軸機器２指令In-position",2,"機器２",3223,"2軸機器２逆転JOG指令"]
[3203,"逆転JOG指令",null,null,2,"機器２",2424,"2軸機器２速度制御中",2,"機器２",3224,"2軸機器２完了信号OFF指令"]
[3204,"完了信号OFF指令",null,null,2,"機器２",2425,"2軸機器２速度・位置Latch",2,"機器２",3225,"2軸機器２速度・位置切替許可"]
[3205,"速度・位置切替許可",null,null,2,"機器２",2426,"2軸機器２零点通過",2,"機器２",3226,"2軸機器２位置決ﾃﾞｰﾀ更新待ち"]
[3206,"位置決ﾃﾞｰﾀ更新待ち",null,null,2,"機器２",2427,"2軸機器２Error検出",2,"機器２",3227,"2軸機器２ｴﾗｰリセット"]
[3207,"ｴﾗｰリセット",null,null,2,"機器２",2428,"2軸機器２ServoError検出",2,"機器２",3228,"2軸機器２ｻｰﾎﾞｴﾗｰリセット"]
[3208,"ｻｰﾎﾞｴﾗｰリセット",null,null,2,"機器２",2429,"2軸機器２原点復帰要求",2,"機器２",3229,"2軸機器２始動時の停止入力無効"]
[3209,"始動時の停止入力無効",null,null,2,"機器２",2430,"2軸機器２原点復帰完了",2,"機器２",3230,"2軸機器２ﾕｰｻﾞ使用不可"]
[3210,"ﾕｰｻﾞ使用不可",null,null,2,"機器２",2431,"2軸機器２FLS 検出",2,"機器２",3231,"2軸機器２ﾕｰｻﾞ使用不可"]
[3211,"ﾕｰｻﾞ使用不可",null,null,2,"機器２",2432,"2軸機器２RLS 検出",2,"機器２",3232,"2軸機器２送り現在値更新指令"]
[3212,"送り現在値更新指令",null,null,2,"機器２",2433,"2軸機器２STOP 検出",2,"機器２",3233,"2軸機器２ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[3213,"ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令",null,null,2,"機器２",2434,"2軸機器２DOG/CHANGE 検出",2,"機器２",3234,"2軸機器２ｶﾑ基準位置設定指令"]
[3214,"ｶﾑ基準位置設定指令",null,null,2,"機器２",2435,"2軸機器２ServoReady",2,"機器２",3235,"2軸機器２ｻｰﾎﾞｵﾌ指令"]
[3215,"ｻｰﾎﾞｵﾌ指令",null,null,2,"機器２",2436,"2軸機器２ﾄﾙｸ制御中",2,"機器２",3236,"2軸機器２ﾕｰｻﾞ使用不可"]
[3216,"ﾕｰｻﾞ使用不可",null,null,2,"機器２",2437,"2軸機器２ﾕｰｻﾞ使用不可",2,"機器２",3237,"2軸機器２ﾕｰｻﾞ使用不可"]
[3217,"ﾕｰｻﾞ使用不可",null,null,2,"機器２",2438,"2軸機器２仮想ﾓｰﾄﾞ継続不可",2,"機器２",3238,"2軸機器２ﾕｰｻﾞ使用不可"]
[3218,"ﾕｰｻﾞ使用不可",null,null,2,"機器２",2439,"2軸機器２Mｺｰﾄﾞ出力中",2,"機器２",3239,"2軸機器２FIN信号"]
[3219,"FIN信号",null,null,3,"機器３",2440,"3軸機器３位置決始動完了",3,"機器３",3240,"3軸機器３停止指令"]
[{"$nulls":4},3,"機器３",2441,"3軸機器３位置決完了",3,"機器３",3241,"3軸機器３急停止指令"]
[{"$nulls":4},3,"機器３",2442,"3軸機器３In-position",3,"機器３",3242,"3軸機器３正転JOG指令"]
[{"$nulls":4},3,"機器３",2443,"3軸機器３指令In-position",3,"機器３",3243,"3軸機器３逆転JOG指令"]
[{"$nulls":4},3,"機器３",2444,"3軸機器３速度制御中",3,"機器３",3244,"3軸機器３完了信号OFF指令"]
[{"$nulls":4},3,"機器３",2445,"3軸機器３速度・位置Latch",3,"機器３",3245,"3軸機器３速度・位置切替許可"]
[{"$nulls":4},3,"機器３",2446,"3軸機器３零点通過",3,"機器３",3246,"3軸機器３位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},3,"機器３",2447,"3軸機器３Error検出",3,"機器３",3247,"3軸機器３ｴﾗｰリセット"]
[{"$nulls":4},3,"機器３",2448,"3軸機器３ServoError検出",3,"機器３",3248,"3軸機器３ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},3,"機器３",2449,"3軸機器３原点復帰要求",3,"機器３",3249,"3軸機器３始動時の停止入力無効"]
[{"$nulls":4},3,"機器３",2450,"3軸機器３原点復帰完了",3,"機器３",3250,"3軸機器３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},3,"機器３",2451,"3軸機器３FLS 検出",3,"機器３",3251,"3軸機器３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},3,"機器３",2452,"3軸機器３RLS 検出",3,"機器３",3252,"3軸機器３送り現在値更新指令"]
[{"$nulls":4},3,"機器３",2453,"3軸機器３STOP 検出",3,"機器３",3253,"3軸機器３ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},3,"機器３",2454,"3軸機器３DOG/CHANGE 検出",3,"機器３",3254,"3軸機器３ｶﾑ基準位置設定指令"]
[{"$nulls":4},3,"機器３",2455,"3軸機器３ServoReady",3,"機器３",3255,"3軸機器３ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},3,"機器３",2456,"3軸機器３ﾄﾙｸ制御中",3,"機器３",3256,"3軸機器３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},3,"機器３",2457,"3軸機器３ﾕｰｻﾞ使用不可",3,"機器３",3257,"3軸機器３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},3,"機器３",2458,"3軸機器３仮想ﾓｰﾄﾞ継続不可",3,"機器３",3258,"3軸機器３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},3,"機器３",2459,"3軸機器３Mｺｰﾄﾞ出力中",3,"機器３",3259,"3軸機器３FIN信号"]
[{"$nulls":4},4,"機器４",2460,"4軸機器４位置決始動完了",4,"機器４",3260,"4軸機器４停止指令"]
[{"$nulls":4},4,"機器４",2461,"4軸機器４位置決完了",4,"機器４",3261,"4軸機器４急停止指令"]
[{"$nulls":4},4,"機器４",2462,"4軸機器４In-position",4,"機器４",3262,"4軸機器４正転JOG指令"]
[{"$nulls":4},4,"機器４",2463,"4軸機器４指令In-position",4,"機器４",3263,"4軸機器４逆転JOG指令"]
[{"$nulls":4},4,"機器４",2464,"4軸機器４速度制御中",4,"機器４",3264,"4軸機器４完了信号OFF指令"]
[{"$nulls":4},4,"機器４",2465,"4軸機器４速度・位置Latch",4,"機器４",3265,"4軸機器４速度・位置切替許可"]
[{"$nulls":4},4,"機器４",2466,"4軸機器４零点通過",4,"機器４",3266,"4軸機器４位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},4,"機器４",2467,"4軸機器４Error検出",4,"機器４",3267,"4軸機器４ｴﾗｰリセット"]
[{"$nulls":4},4,"機器４",2468,"4軸機器４ServoError検出",4,"機器４",3268,"4軸機器４ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},4,"機器４",2469,"4軸機器４原点復帰要求",4,"機器４",3269,"4軸機器４始動時の停止入力無効"]
[{"$nulls":4},4,"機器４",2470,"4軸機器４原点復帰完了",4,"機器４",3270,"4軸機器４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},4,"機器４",2471,"4軸機器４FLS 検出",4,"機器４",3271,"4軸機器４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},4,"機器４",2472,"4軸機器４RLS 検出",4,"機器４",3272,"4軸機器４送り現在値更新指令"]
[{"$nulls":4},4,"機器４",2473,"4軸機器４STOP 検出",4,"機器４",3273,"4軸機器４ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},4,"機器４",2474,"4軸機器４DOG/CHANGE 検出",4,"機器４",3274,"4軸機器４ｶﾑ基準位置設定指令"]
[{"$nulls":4},4,"機器４",2475,"4軸機器４ServoReady",4,"機器４",3275,"4軸機器４ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},4,"機器４",2476,"4軸機器４ﾄﾙｸ制御中",4,"機器４",3276,"4軸機器４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},4,"機器４",2477,"4軸機器４ﾕｰｻﾞ使用不可",4,"機器４",3277,"4軸機器４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},4,"機器４",2478,"4軸機器４仮想ﾓｰﾄﾞ継続不可",4,"機器４",3278,"4軸機器４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},4,"機器４",2479,"4軸機器４Mｺｰﾄﾞ出力中",4,"機器４",3279,"4軸機器４FIN信号"]
[{"$nulls":4},5,"機器５",2480,"5軸機器５位置決始動完了",5,"機器５",3280,"5軸機器５停止指令"]
[{"$nulls":4},5,"機器５",2481,"5軸機器５位置決完了",5,"機器５",3281,"5軸機器５急停止指令"]
[{"$nulls":4},5,"機器５",2482,"5軸機器５In-position",5,"機器５",3282,"5軸機器５正転JOG指令"]
[{"$nulls":4},5,"機器５",2483,"5軸機器５指令In-position",5,"機器５",3283,"5軸機器５逆転JOG指令"]
[{"$nulls":4},5,"機器５",2484,"5軸機器５速度制御中",5,"機器５",3284,"5軸機器５完了信号OFF指令"]
[{"$nulls":4},5,"機器５",2485,"5軸機器５速度・位置Latch",5,"機器５",3285,"5軸機器５速度・位置切替許可"]
[{"$nulls":4},5,"機器５",2486,"5軸機器５零点通過",5,"機器５",3286,"5軸機器５位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},5,"機器５",2487,"5軸機器５Error検出",5,"機器５",3287,"5軸機器５ｴﾗｰリセット"]
[{"$nulls":4},5,"機器５",2488,"5軸機器５ServoError検出",5,"機器５",3288,"5軸機器５ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},5,"機器５",2489,"5軸機器５原点復帰要求",5,"機器５",3289,"5軸機器５始動時の停止入力無効"]
[{"$nulls":4},5,"機器５",2490,"5軸機器５原点復帰完了",5,"機器５",3290,"5軸機器５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},5,"機器５",2491,"5軸機器５FLS 検出",5,"機器５",3291,"5軸機器５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},5,"機器５",2492,"5軸機器５RLS 検出",5,"機器５",3292,"5軸機器５送り現在値更新指令"]
[{"$nulls":4},5,"機器５",2493,"5軸機器５STOP 検出",5,"機器５",3293,"5軸機器５ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},5,"機器５",2494,"5軸機器５DOG/CHANGE 検出",5,"機器５",3294,"5軸機器５ｶﾑ基準位置設定指令"]
[{"$nulls":4},5,"機器５",2495,"5軸機器５ServoReady",5,"機器５",3295,"5軸機器５ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},5,"機器５",2496,"5軸機器５ﾄﾙｸ制御中",5,"機器５",3296,"5軸機器５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},5,"機器５",2497,"5軸機器５ﾕｰｻﾞ使用不可",5,"機器５",3297,"5軸機器５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},5,"機器５",2498,"5軸機器５仮想ﾓｰﾄﾞ継続不可",5,"機器５",3298,"5軸機器５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},5,"機器５",2499,"5軸機器５Mｺｰﾄﾞ出力中",5,"機器５",3299,"5軸機器５FIN信号"]
[{"$nulls":4},6,"機器６",2500,"6軸機器６位置決始動完了",6,"機器６",3300,"6軸機器６停止指令"]
[{"$nulls":4},6,"機器６",2501,"6軸機器６位置決完了",6,"機器６",3301,"6軸機器６急停止指令"]
[{"$nulls":4},6,"機器６",2502,"6軸機器６In-position",6,"機器６",3302,"6軸機器６正転JOG指令"]
[{"$nulls":4},6,"機器６",2503,"6軸機器６指令In-position",6,"機器６",3303,"6軸機器６逆転JOG指令"]
[{"$nulls":4},6,"機器６",2504,"6軸機器６速度制御中",6,"機器６",3304,"6軸機器６完了信号OFF指令"]
[{"$nulls":4},6,"機器６",2505,"6軸機器６速度・位置Latch",6,"機器６",3305,"6軸機器６速度・位置切替許可"]
[{"$nulls":4},6,"機器６",2506,"6軸機器６零点通過",6,"機器６",3306,"6軸機器６位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},6,"機器６",2507,"6軸機器６Error検出",6,"機器６",3307,"6軸機器６ｴﾗｰリセット"]
[{"$nulls":4},6,"機器６",2508,"6軸機器６ServoError検出",6,"機器６",3308,"6軸機器６ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},6,"機器６",2509,"6軸機器６原点復帰要求",6,"機器６",3309,"6軸機器６始動時の停止入力無効"]
[{"$nulls":4},6,"機器６",2510,"6軸機器６原点復帰完了",6,"機器６",3310,"6軸機器６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},6,"機器６",2511,"6軸機器６FLS 検出",6,"機器６",3311,"6軸機器６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},6,"機器６",2512,"6軸機器６RLS 検出",6,"機器６",3312,"6軸機器６送り現在値更新指令"]
[{"$nulls":4},6,"機器６",2513,"6軸機器６STOP 検出",6,"機器６",3313,"6軸機器６ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},6,"機器６",2514,"6軸機器６DOG/CHANGE 検出",6,"機器６",3314,"6軸機器６ｶﾑ基準位置設定指令"]
[{"$nulls":4},6,"機器６",2515,"6軸機器６ServoReady",6,"機器６",3315,"6軸機器６ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},6,"機器６",2516,"6軸機器６ﾄﾙｸ制御中",6,"機器６",3316,"6軸機器６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},6,"機器６",2517,"6軸機器６ﾕｰｻﾞ使用不可",6,"機器６",3317,"6軸機器６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},6,"機器６",2518,"6軸機器６仮想ﾓｰﾄﾞ継続不可",6,"機器６",3318,"6軸機器６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},6,"機器６",2519,"6軸機器６Mｺｰﾄﾞ出力中",6,"機器６",3319,"6軸機器６FIN信号"]
[{"$nulls":4},7,"機器７",2520,"7軸機器７位置決始動完了",7,"機器７",3320,"7軸機器７停止指令"]
[{"$nulls":4},7,"機器７",2521,"7軸機器７位置決完了",7,"機器７",3321,"7軸機器７急停止指令"]
[{"$nulls":4},7,"機器７",2522,"7軸機器７In-position",7,"機器７",3322,"7軸機器７正転JOG指令"]
[{"$nulls":4},7,"機器７",2523,"7軸機器７指令In-position",7,"機器７",3323,"7軸機器７逆転JOG指令"]
[{"$nulls":4},7,"機器７",2524,"7軸機器７速度制御中",7,"機器７",3324,"7軸機器７完了信号OFF指令"]
[{"$nulls":4},7,"機器７",2525,"7軸機器７速度・位置Latch",7,"機器７",3325,"7軸機器７速度・位置切替許可"]
[{"$nulls":4},7,"機器７",2526,"7軸機器７零点通過",7,"機器７",3326,"7軸機器７位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},7,"機器７",2527,"7軸機器７Error検出",7,"機器７",3327,"7軸機器７ｴﾗｰリセット"]
[{"$nulls":4},7,"機器７",2528,"7軸機器７ServoError検出",7,"機器７",3328,"7軸機器７ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},7,"機器７",2529,"7軸機器７原点復帰要求",7,"機器７",3329,"7軸機器７始動時の停止入力無効"]
[{"$nulls":4},7,"機器７",2530,"7軸機器７原点復帰完了",7,"機器７",3330,"7軸機器７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},7,"機器７",2531,"7軸機器７FLS 検出",7,"機器７",3331,"7軸機器７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},7,"機器７",2532,"7軸機器７RLS 検出",7,"機器７",3332,"7軸機器７送り現在値更新指令"]
[{"$nulls":4},7,"機器７",2533,"7軸機器７STOP 検出",7,"機器７",3333,"7軸機器７ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},7,"機器７",2534,"7軸機器７DOG/CHANGE 検出",7,"機器７",3334,"7軸機器７ｶﾑ基準位置設定指令"]
[{"$nulls":4},7,"機器７",2535,"7軸機器７ServoReady",7,"機器７",3335,"7軸機器７ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},7,"機器７",2536,"7軸機器７ﾄﾙｸ制御中",7,"機器７",3336,"7軸機器７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},7,"機器７",2537,"7軸機器７ﾕｰｻﾞ使用不可",7,"機器７",3337,"7軸機器７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},7,"機器７",2538,"7軸機器７仮想ﾓｰﾄﾞ継続不可",7,"機器７",3338,"7軸機器７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},7,"機器７",2539,"7軸機器７Mｺｰﾄﾞ出力中",7,"機器７",3339,"7軸機器７FIN信号"]
[{"$nulls":4},8,"機器８",2540,"8軸機器８位置決始動完了",8,"機器８",3340,"8軸機器８停止指令"]
[{"$nulls":4},8,"機器８",2541,"8軸機器８位置決完了",8,"機器８",3341,"8軸機器８急停止指令"]
[{"$nulls":4},8,"機器８",2542,"8軸機器８In-position",8,"機器８",3342,"8軸機器８正転JOG指令"]
[{"$nulls":4},8,"機器８",2543,"8軸機器８指令In-position",8,"機器８",3343,"8軸機器８逆転JOG指令"]
[{"$nulls":4},8,"機器８",2544,"8軸機器８速度制御中",8,"機器８",3344,"8軸機器８完了信号OFF指令"]
[{"$nulls":4},8,"機器８",2545,"8軸機器８速度・位置Latch",8,"機器８",3345,"8軸機器８速度・位置切替許可"]
[{"$nulls":4},8,"機器８",2546,"8軸機器８零点通過",8,"機器８",3346,"8軸機器８位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},8,"機器８",2547,"8軸機器８Error検出",8,"機器８",3347,"8軸機器８ｴﾗｰリセット"]
[{"$nulls":4},8,"機器８",2548,"8軸機器８ServoError検出",8,"機器８",3348,"8軸機器８ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},8,"機器８",2549,"8軸機器８原点復帰要求",8,"機器８",3349,"8軸機器８始動時の停止入力無効"]
[{"$nulls":4},8,"機器８",2550,"8軸機器８原点復帰完了",8,"機器８",3350,"8軸機器８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},8,"機器８",2551,"8軸機器８FLS 検出",8,"機器８",3351,"8軸機器８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},8,"機器８",2552,"8軸機器８RLS 検出",8,"機器８",3352,"8軸機器８送り現在値更新指令"]
[{"$nulls":4},8,"機器８",2553,"8軸機器８STOP 検出",8,"機器８",3353,"8軸機器８ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},8,"機器８",2554,"8軸機器８DOG/CHANGE 検出",8,"機器８",3354,"8軸機器８ｶﾑ基準位置設定指令"]
[{"$nulls":4},8,"機器８",2555,"8軸機器８ServoReady",8,"機器８",3355,"8軸機器８ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},8,"機器８",2556,"8軸機器８ﾄﾙｸ制御中",8,"機器８",3356,"8軸機器８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},8,"機器８",2557,"8軸機器８ﾕｰｻﾞ使用不可",8,"機器８",3357,"8軸機器８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},8,"機器８",2558,"8軸機器８仮想ﾓｰﾄﾞ継続不可",8,"機器８",3358,"8軸機器８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},8,"機器８",2559,"8軸機器８Mｺｰﾄﾞ出力中",8,"機器８",3359,"8軸機器８FIN信号"]
[{"$nulls":4},9,"機器９",2560,"9軸機器９位置決始動完了",9,"機器９",3360,"9軸機器９停止指令"]
[{"$nulls":4},9,"機器９",2561,"9軸機器９位置決完了",9,"機器９",3361,"9軸機器９急停止指令"]
[{"$nulls":4},9,"機器９",2562,"9軸機器９In-position",9,"機器９",3362,"9軸機器９正転JOG指令"]
[{"$nulls":4},9,"機器９",2563,"9軸機器９指令In-position",9,"機器９",3363,"9軸機器９逆転JOG指令"]
[{"$nulls":4},9,"機器９",2564,"9軸機器９速度制御中",9,"機器９",3364,"9軸機器９完了信号OFF指令"]
[{"$nulls":4},9,"機器９",2565,"9軸機器９速度・位置Latch",9,"機器９",3365,"9軸機器９速度・位置切替許可"]
[{"$nulls":4},9,"機器９",2566,"9軸機器９零点通過",9,"機器９",3366,"9軸機器９位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},9,"機器９",2567,"9軸機器９Error検出",9,"機器９",3367,"9軸機器９ｴﾗｰリセット"]
[{"$nulls":4},9,"機器９",2568,"9軸機器９ServoError検出",9,"機器９",3368,"9軸機器９ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},9,"機器９",2569,"9軸機器９原点復帰要求",9,"機器９",3369,"9軸機器９始動時の停止入力無効"]
[{"$nulls":4},9,"機器９",2570,"9軸機器９原点復帰完了",9,"機器９",3370,"9軸機器９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},9,"機器９",2571,"9軸機器９FLS 検出",9,"機器９",3371,"9軸機器９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},9,"機器９",2572,"9軸機器９RLS 検出",9,"機器９",3372,"9軸機器９送り現在値更新指令"]
[{"$nulls":4},9,"機器９",2573,"9軸機器９STOP 検出",9,"機器９",3373,"9軸機器９ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},9,"機器９",2574,"9軸機器９DOG/CHANGE 検出",9,"機器９",3374,"9軸機器９ｶﾑ基準位置設定指令"]
[{"$nulls":4},9,"機器９",2575,"9軸機器９ServoReady",9,"機器９",3375,"9軸機器９ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},9,"機器９",2576,"9軸機器９ﾄﾙｸ制御中",9,"機器９",3376,"9軸機器９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},9,"機器９",2577,"9軸機器９ﾕｰｻﾞ使用不可",9,"機器９",3377,"9軸機器９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},9,"機器９",2578,"9軸機器９仮想ﾓｰﾄﾞ継続不可",9,"機器９",3378,"9軸機器９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},9,"機器９",2579,"9軸機器９Mｺｰﾄﾞ出力中",9,"機器９",3379,"9軸機器９FIN信号"]
[{"$nulls":4},10,"機器１０",2580,"10軸機器１０位置決始動完了",10,"機器１０",3380,"10軸機器１０停止指令"]
[{"$nulls":4},10,"機器１０",2581,"10軸機器１０位置決完了",10,"機器１０",3381,"10軸機器１０急停止指令"]
[{"$nulls":4},10,"機器１０",2582,"10軸機器１０In-position",10,"機器１０",3382,"10軸機器１０正転JOG指令"]
[{"$nulls":4},10,"機器１０",2583,"10軸機器１０指令In-position",10,"機器１０",3383,"10軸機器１０逆転JOG指令"]
[{"$nulls":4},10,"機器１０",2584,"10軸機器１０速度制御中",10,"機器１０",3384,"10軸機器１０完了信号OFF指令"]
[{"$nulls":4},10,"機器１０",2585,"10軸機器１０速度・位置Latch",10,"機器１０",3385,"10軸機器１０速度・位置切替許可"]
[{"$nulls":4},10,"機器１０",2586,"10軸機器１０零点通過",10,"機器１０",3386,"10軸機器１０位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},10,"機器１０",2587,"10軸機器１０Error検出",10,"機器１０",3387,"10軸機器１０ｴﾗｰリセット"]
[{"$nulls":4},10,"機器１０",2588,"10軸機器１０ServoError検出",10,"機器１０",3388,"10軸機器１０ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},10,"機器１０",2589,"10軸機器１０原点復帰要求",10,"機器１０",3389,"10軸機器１０始動時の停止入力無効"]
[{"$nulls":4},10,"機器１０",2590,"10軸機器１０原点復帰完了",10,"機器１０",3390,"10軸機器１０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},10,"機器１０",2591,"10軸機器１０FLS 検出",10,"機器１０",3391,"10軸機器１０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},10,"機器１０",2592,"10軸機器１０RLS 検出",10,"機器１０",3392,"10軸機器１０送り現在値更新指令"]
[{"$nulls":4},10,"機器１０",2593,"10軸機器１０STOP 検出",10,"機器１０",3393,"10軸機器１０ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},10,"機器１０",2594,"10軸機器１０DOG/CHANGE 検出",10,"機器１０",3394,"10軸機器１０ｶﾑ基準位置設定指令"]
[{"$nulls":4},10,"機器１０",2595,"10軸機器１０ServoReady",10,"機器１０",3395,"10軸機器１０ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},10,"機器１０",2596,"10軸機器１０ﾄﾙｸ制御中",10,"機器１０",3396,"10軸機器１０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},10,"機器１０",2597,"10軸機器１０ﾕｰｻﾞ使用不可",10,"機器１０",3397,"10軸機器１０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},10,"機器１０",2598,"10軸機器１０仮想ﾓｰﾄﾞ継続不可",10,"機器１０",3398,"10軸機器１０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},10,"機器１０",2599,"10軸機器１０Mｺｰﾄﾞ出力中",10,"機器１０",3399,"10軸機器１０FIN信号"]
[{"$nulls":4},11,"機器１１",2600,"11軸機器１１位置決始動完了",11,"機器１１",3400,"11軸機器１１停止指令"]
[{"$nulls":4},11,"機器１１",2601,"11軸機器１１位置決完了",11,"機器１１",3401,"11軸機器１１急停止指令"]
[{"$nulls":4},11,"機器１１",2602,"11軸機器１１In-position",11,"機器１１",3402,"11軸機器１１正転JOG指令"]
[{"$nulls":4},11,"機器１１",2603,"11軸機器１１指令In-position",11,"機器１１",3403,"11軸機器１１逆転JOG指令"]
[{"$nulls":4},11,"機器１１",2604,"11軸機器１１速度制御中",11,"機器１１",3404,"11軸機器１１完了信号OFF指令"]
[{"$nulls":4},11,"機器１１",2605,"11軸機器１１速度・位置Latch",11,"機器１１",3405,"11軸機器１１速度・位置切替許可"]
[{"$nulls":4},11,"機器１１",2606,"11軸機器１１零点通過",11,"機器１１",3406,"11軸機器１１位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},11,"機器１１",2607,"11軸機器１１Error検出",11,"機器１１",3407,"11軸機器１１ｴﾗｰリセット"]
[{"$nulls":4},11,"機器１１",2608,"11軸機器１１ServoError検出",11,"機器１１",3408,"11軸機器１１ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},11,"機器１１",2609,"11軸機器１１原点復帰要求",11,"機器１１",3409,"11軸機器１１始動時の停止入力無効"]
[{"$nulls":4},11,"機器１１",2610,"11軸機器１１原点復帰完了",11,"機器１１",3410,"11軸機器１１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},11,"機器１１",2611,"11軸機器１１FLS 検出",11,"機器１１",3411,"11軸機器１１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},11,"機器１１",2612,"11軸機器１１RLS 検出",11,"機器１１",3412,"11軸機器１１送り現在値更新指令"]
[{"$nulls":4},11,"機器１１",2613,"11軸機器１１STOP 検出",11,"機器１１",3413,"11軸機器１１ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},11,"機器１１",2614,"11軸機器１１DOG/CHANGE 検出",11,"機器１１",3414,"11軸機器１１ｶﾑ基準位置設定指令"]
[{"$nulls":4},11,"機器１１",2615,"11軸機器１１ServoReady",11,"機器１１",3415,"11軸機器１１ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},11,"機器１１",2616,"11軸機器１１ﾄﾙｸ制御中",11,"機器１１",3416,"11軸機器１１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},11,"機器１１",2617,"11軸機器１１ﾕｰｻﾞ使用不可",11,"機器１１",3417,"11軸機器１１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},11,"機器１１",2618,"11軸機器１１仮想ﾓｰﾄﾞ継続不可",11,"機器１１",3418,"11軸機器１１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},11,"機器１１",2619,"11軸機器１１Mｺｰﾄﾞ出力中",11,"機器１１",3419,"11軸機器１１FIN信号"]
[{"$nulls":4},12,"機器１２",2620,"12軸機器１２位置決始動完了",12,"機器１２",3420,"12軸機器１２停止指令"]
[{"$nulls":4},12,"機器１２",2621,"12軸機器１２位置決完了",12,"機器１２",3421,"12軸機器１２急停止指令"]
[{"$nulls":4},12,"機器１２",2622,"12軸機器１２In-position",12,"機器１２",3422,"12軸機器１２正転JOG指令"]
[{"$nulls":4},12,"機器１２",2623,"12軸機器１２指令In-position",12,"機器１２",3423,"12軸機器１２逆転JOG指令"]
[{"$nulls":4},12,"機器１２",2624,"12軸機器１２速度制御中",12,"機器１２",3424,"12軸機器１２完了信号OFF指令"]
[{"$nulls":4},12,"機器１２",2625,"12軸機器１２速度・位置Latch",12,"機器１２",3425,"12軸機器１２速度・位置切替許可"]
[{"$nulls":4},12,"機器１２",2626,"12軸機器１２零点通過",12,"機器１２",3426,"12軸機器１２位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},12,"機器１２",2627,"12軸機器１２Error検出",12,"機器１２",3427,"12軸機器１２ｴﾗｰリセット"]
[{"$nulls":4},12,"機器１２",2628,"12軸機器１２ServoError検出",12,"機器１２",3428,"12軸機器１２ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},12,"機器１２",2629,"12軸機器１２原点復帰要求",12,"機器１２",3429,"12軸機器１２始動時の停止入力無効"]
[{"$nulls":4},12,"機器１２",2630,"12軸機器１２原点復帰完了",12,"機器１２",3430,"12軸機器１２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},12,"機器１２",2631,"12軸機器１２FLS 検出",12,"機器１２",3431,"12軸機器１２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},12,"機器１２",2632,"12軸機器１２RLS 検出",12,"機器１２",3432,"12軸機器１２送り現在値更新指令"]
[{"$nulls":4},12,"機器１２",2633,"12軸機器１２STOP 検出",12,"機器１２",3433,"12軸機器１２ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},12,"機器１２",2634,"12軸機器１２DOG/CHANGE 検出",12,"機器１２",3434,"12軸機器１２ｶﾑ基準位置設定指令"]
[{"$nulls":4},12,"機器１２",2635,"12軸機器１２ServoReady",12,"機器１２",3435,"12軸機器１２ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},12,"機器１２",2636,"12軸機器１２ﾄﾙｸ制御中",12,"機器１２",3436,"12軸機器１２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},12,"機器１２",2637,"12軸機器１２ﾕｰｻﾞ使用不可",12,"機器１２",3437,"12軸機器１２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},12,"機器１２",2638,"12軸機器１２仮想ﾓｰﾄﾞ継続不可",12,"機器１２",3438,"12軸機器１２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},12,"機器１２",2639,"12軸機器１２Mｺｰﾄﾞ出力中",12,"機器１２",3439,"12軸機器１２FIN信号"]
[{"$nulls":4},13,"機器１３",2640,"13軸機器１３位置決始動完了",13,"機器１３",3440,"13軸機器１３停止指令"]
[{"$nulls":4},13,"機器１３",2641,"13軸機器１３位置決完了",13,"機器１３",3441,"13軸機器１３急停止指令"]
[{"$nulls":4},13,"機器１３",2642,"13軸機器１３In-position",13,"機器１３",3442,"13軸機器１３正転JOG指令"]
[{"$nulls":4},13,"機器１３",2643,"13軸機器１３指令In-position",13,"機器１３",3443,"13軸機器１３逆転JOG指令"]
[{"$nulls":4},13,"機器１３",2644,"13軸機器１３速度制御中",13,"機器１３",3444,"13軸機器１３完了信号OFF指令"]
[{"$nulls":4},13,"機器１３",2645,"13軸機器１３速度・位置Latch",13,"機器１３",3445,"13軸機器１３速度・位置切替許可"]
[{"$nulls":4},13,"機器１３",2646,"13軸機器１３零点通過",13,"機器１３",3446,"13軸機器１３位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},13,"機器１３",2647,"13軸機器１３Error検出",13,"機器１３",3447,"13軸機器１３ｴﾗｰリセット"]
[{"$nulls":4},13,"機器１３",2648,"13軸機器１３ServoError検出",13,"機器１３",3448,"13軸機器１３ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},13,"機器１３",2649,"13軸機器１３原点復帰要求",13,"機器１３",3449,"13軸機器１３始動時の停止入力無効"]
[{"$nulls":4},13,"機器１３",2650,"13軸機器１３原点復帰完了",13,"機器１３",3450,"13軸機器１３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},13,"機器１３",2651,"13軸機器１３FLS 検出",13,"機器１３",3451,"13軸機器１３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},13,"機器１３",2652,"13軸機器１３RLS 検出",13,"機器１３",3452,"13軸機器１３送り現在値更新指令"]
[{"$nulls":4},13,"機器１３",2653,"13軸機器１３STOP 検出",13,"機器１３",3453,"13軸機器１３ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},13,"機器１３",2654,"13軸機器１３DOG/CHANGE 検出",13,"機器１３",3454,"13軸機器１３ｶﾑ基準位置設定指令"]
[{"$nulls":4},13,"機器１３",2655,"13軸機器１３ServoReady",13,"機器１３",3455,"13軸機器１３ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},13,"機器１３",2656,"13軸機器１３ﾄﾙｸ制御中",13,"機器１３",3456,"13軸機器１３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},13,"機器１３",2657,"13軸機器１３ﾕｰｻﾞ使用不可",13,"機器１３",3457,"13軸機器１３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},13,"機器１３",2658,"13軸機器１３仮想ﾓｰﾄﾞ継続不可",13,"機器１３",3458,"13軸機器１３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},13,"機器１３",2659,"13軸機器１３Mｺｰﾄﾞ出力中",13,"機器１３",3459,"13軸機器１３FIN信号"]
[{"$nulls":4},14,"機器１４",2660,"14軸機器１４位置決始動完了",14,"機器１４",3460,"14軸機器１４停止指令"]
[{"$nulls":4},14,"機器１４",2661,"14軸機器１４位置決完了",14,"機器１４",3461,"14軸機器１４急停止指令"]
[{"$nulls":4},14,"機器１４",2662,"14軸機器１４In-position",14,"機器１４",3462,"14軸機器１４正転JOG指令"]
[{"$nulls":4},14,"機器１４",2663,"14軸機器１４指令In-position",14,"機器１４",3463,"14軸機器１４逆転JOG指令"]
[{"$nulls":4},14,"機器１４",2664,"14軸機器１４速度制御中",14,"機器１４",3464,"14軸機器１４完了信号OFF指令"]
[{"$nulls":4},14,"機器１４",2665,"14軸機器１４速度・位置Latch",14,"機器１４",3465,"14軸機器１４速度・位置切替許可"]
[{"$nulls":4},14,"機器１４",2666,"14軸機器１４零点通過",14,"機器１４",3466,"14軸機器１４位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},14,"機器１４",2667,"14軸機器１４Error検出",14,"機器１４",3467,"14軸機器１４ｴﾗｰリセット"]
[{"$nulls":4},14,"機器１４",2668,"14軸機器１４ServoError検出",14,"機器１４",3468,"14軸機器１４ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},14,"機器１４",2669,"14軸機器１４原点復帰要求",14,"機器１４",3469,"14軸機器１４始動時の停止入力無効"]
[{"$nulls":4},14,"機器１４",2670,"14軸機器１４原点復帰完了",14,"機器１４",3470,"14軸機器１４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},14,"機器１４",2671,"14軸機器１４FLS 検出",14,"機器１４",3471,"14軸機器１４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},14,"機器１４",2672,"14軸機器１４RLS 検出",14,"機器１４",3472,"14軸機器１４送り現在値更新指令"]
[{"$nulls":4},14,"機器１４",2673,"14軸機器１４STOP 検出",14,"機器１４",3473,"14軸機器１４ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},14,"機器１４",2674,"14軸機器１４DOG/CHANGE 検出",14,"機器１４",3474,"14軸機器１４ｶﾑ基準位置設定指令"]
[{"$nulls":4},14,"機器１４",2675,"14軸機器１４ServoReady",14,"機器１４",3475,"14軸機器１４ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},14,"機器１４",2676,"14軸機器１４ﾄﾙｸ制御中",14,"機器１４",3476,"14軸機器１４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},14,"機器１４",2677,"14軸機器１４ﾕｰｻﾞ使用不可",14,"機器１４",3477,"14軸機器１４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},14,"機器１４",2678,"14軸機器１４仮想ﾓｰﾄﾞ継続不可",14,"機器１４",3478,"14軸機器１４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},14,"機器１４",2679,"14軸機器１４Mｺｰﾄﾞ出力中",14,"機器１４",3479,"14軸機器１４FIN信号"]
[{"$nulls":4},15,"機器１５",2680,"15軸機器１５位置決始動完了",15,"機器１５",3480,"15軸機器１５停止指令"]
[{"$nulls":4},15,"機器１５",2681,"15軸機器１５位置決完了",15,"機器１５",3481,"15軸機器１５急停止指令"]
[{"$nulls":4},15,"機器１５",2682,"15軸機器１５In-position",15,"機器１５",3482,"15軸機器１５正転JOG指令"]
[{"$nulls":4},15,"機器１５",2683,"15軸機器１５指令In-position",15,"機器１５",3483,"15軸機器１５逆転JOG指令"]
[{"$nulls":4},15,"機器１５",2684,"15軸機器１５速度制御中",15,"機器１５",3484,"15軸機器１５完了信号OFF指令"]
[{"$nulls":4},15,"機器１５",2685,"15軸機器１５速度・位置Latch",15,"機器１５",3485,"15軸機器１５速度・位置切替許可"]
[{"$nulls":4},15,"機器１５",2686,"15軸機器１５零点通過",15,"機器１５",3486,"15軸機器１５位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},15,"機器１５",2687,"15軸機器１５Error検出",15,"機器１５",3487,"15軸機器１５ｴﾗｰリセット"]
[{"$nulls":4},15,"機器１５",2688,"15軸機器１５ServoError検出",15,"機器１５",3488,"15軸機器１５ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},15,"機器１５",2689,"15軸機器１５原点復帰要求",15,"機器１５",3489,"15軸機器１５始動時の停止入力無効"]
[{"$nulls":4},15,"機器１５",2690,"15軸機器１５原点復帰完了",15,"機器１５",3490,"15軸機器１５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},15,"機器１５",2691,"15軸機器１５FLS 検出",15,"機器１５",3491,"15軸機器１５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},15,"機器１５",2692,"15軸機器１５RLS 検出",15,"機器１５",3492,"15軸機器１５送り現在値更新指令"]
[{"$nulls":4},15,"機器１５",2693,"15軸機器１５STOP 検出",15,"機器１５",3493,"15軸機器１５ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},15,"機器１５",2694,"15軸機器１５DOG/CHANGE 検出",15,"機器１５",3494,"15軸機器１５ｶﾑ基準位置設定指令"]
[{"$nulls":4},15,"機器１５",2695,"15軸機器１５ServoReady",15,"機器１５",3495,"15軸機器１５ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},15,"機器１５",2696,"15軸機器１５ﾄﾙｸ制御中",15,"機器１５",3496,"15軸機器１５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},15,"機器１５",2697,"15軸機器１５ﾕｰｻﾞ使用不可",15,"機器１５",3497,"15軸機器１５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},15,"機器１５",2698,"15軸機器１５仮想ﾓｰﾄﾞ継続不可",15,"機器１５",3498,"15軸機器１５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},15,"機器１５",2699,"15軸機器１５Mｺｰﾄﾞ出力中",15,"機器１５",3499,"15軸機器１５FIN信号"]
[{"$nulls":4},16,"機器１６",2700,"16軸機器１６位置決始動完了",16,"機器１６",3500,"16軸機器１６停止指令"]
[{"$nulls":4},16,"機器１６",2701,"16軸機器１６位置決完了",16,"機器１６",3501,"16軸機器１６急停止指令"]
[{"$nulls":4},16,"機器１６",2702,"16軸機器１６In-position",16,"機器１６",3502,"16軸機器１６正転JOG指令"]
[{"$nulls":4},16,"機器１６",2703,"16軸機器１６指令In-position",16,"機器１６",3503,"16軸機器１６逆転JOG指令"]
[{"$nulls":4},16,"機器１６",2704,"16軸機器１６速度制御中",16,"機器１６",3504,"16軸機器１６完了信号OFF指令"]
[{"$nulls":4},16,"機器１６",2705,"16軸機器１６速度・位置Latch",16,"機器１６",3505,"16軸機器１６速度・位置切替許可"]
[{"$nulls":4},16,"機器１６",2706,"16軸機器１６零点通過",16,"機器１６",3506,"16軸機器１６位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},16,"機器１６",2707,"16軸機器１６Error検出",16,"機器１６",3507,"16軸機器１６ｴﾗｰリセット"]
[{"$nulls":4},16,"機器１６",2708,"16軸機器１６ServoError検出",16,"機器１６",3508,"16軸機器１６ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},16,"機器１６",2709,"16軸機器１６原点復帰要求",16,"機器１６",3509,"16軸機器１６始動時の停止入力無効"]
[{"$nulls":4},16,"機器１６",2710,"16軸機器１６原点復帰完了",16,"機器１６",3510,"16軸機器１６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},16,"機器１６",2711,"16軸機器１６FLS 検出",16,"機器１６",3511,"16軸機器１６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},16,"機器１６",2712,"16軸機器１６RLS 検出",16,"機器１６",3512,"16軸機器１６送り現在値更新指令"]
[{"$nulls":4},16,"機器１６",2713,"16軸機器１６STOP 検出",16,"機器１６",3513,"16軸機器１６ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},16,"機器１６",2714,"16軸機器１６DOG/CHANGE 検出",16,"機器１６",3514,"16軸機器１６ｶﾑ基準位置設定指令"]
[{"$nulls":4},16,"機器１６",2715,"16軸機器１６ServoReady",16,"機器１６",3515,"16軸機器１６ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},16,"機器１６",2716,"16軸機器１６ﾄﾙｸ制御中",16,"機器１６",3516,"16軸機器１６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},16,"機器１６",2717,"16軸機器１６ﾕｰｻﾞ使用不可",16,"機器１６",3517,"16軸機器１６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},16,"機器１６",2718,"16軸機器１６仮想ﾓｰﾄﾞ継続不可",16,"機器１６",3518,"16軸機器１６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},16,"機器１６",2719,"16軸機器１６Mｺｰﾄﾞ出力中",16,"機器１６",3519,"16軸機器１６FIN信号"]
[{"$nulls":4},17,"機器１７",2720,"17軸機器１７位置決始動完了",17,"機器１７",3520,"17軸機器１７停止指令"]
[{"$nulls":4},17,"機器１７",2721,"17軸機器１７位置決完了",17,"機器１７",3521,"17軸機器１７急停止指令"]
[{"$nulls":4},17,"機器１７",2722,"17軸機器１７In-position",17,"機器１７",3522,"17軸機器１７正転JOG指令"]
[{"$nulls":4},17,"機器１７",2723,"17軸機器１７指令In-position",17,"機器１７",3523,"17軸機器１７逆転JOG指令"]
[{"$nulls":4},17,"機器１７",2724,"17軸機器１７速度制御中",17,"機器１７",3524,"17軸機器１７完了信号OFF指令"]
[{"$nulls":4},17,"機器１７",2725,"17軸機器１７速度・位置Latch",17,"機器１７",3525,"17軸機器１７速度・位置切替許可"]
[{"$nulls":4},17,"機器１７",2726,"17軸機器１７零点通過",17,"機器１７",3526,"17軸機器１７位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},17,"機器１７",2727,"17軸機器１７Error検出",17,"機器１７",3527,"17軸機器１７ｴﾗｰリセット"]
[{"$nulls":4},17,"機器１７",2728,"17軸機器１７ServoError検出",17,"機器１７",3528,"17軸機器１７ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},17,"機器１７",2729,"17軸機器１７原点復帰要求",17,"機器１７",3529,"17軸機器１７始動時の停止入力無効"]
[{"$nulls":4},17,"機器１７",2730,"17軸機器１７原点復帰完了",17,"機器１７",3530,"17軸機器１７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},17,"機器１７",2731,"17軸機器１７FLS 検出",17,"機器１７",3531,"17軸機器１７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},17,"機器１７",2732,"17軸機器１７RLS 検出",17,"機器１７",3532,"17軸機器１７送り現在値更新指令"]
[{"$nulls":4},17,"機器１７",2733,"17軸機器１７STOP 検出",17,"機器１７",3533,"17軸機器１７ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},17,"機器１７",2734,"17軸機器１７DOG/CHANGE 検出",17,"機器１７",3534,"17軸機器１７ｶﾑ基準位置設定指令"]
[{"$nulls":4},17,"機器１７",2735,"17軸機器１７ServoReady",17,"機器１７",3535,"17軸機器１７ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},17,"機器１７",2736,"17軸機器１７ﾄﾙｸ制御中",17,"機器１７",3536,"17軸機器１７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},17,"機器１７",2737,"17軸機器１７ﾕｰｻﾞ使用不可",17,"機器１７",3537,"17軸機器１７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},17,"機器１７",2738,"17軸機器１７仮想ﾓｰﾄﾞ継続不可",17,"機器１７",3538,"17軸機器１７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},17,"機器１７",2739,"17軸機器１７Mｺｰﾄﾞ出力中",17,"機器１７",3539,"17軸機器１７FIN信号"]
[{"$nulls":4},18,"機器１８",2740,"18軸機器１８位置決始動完了",18,"機器１８",3540,"18軸機器１８停止指令"]
[{"$nulls":4},18,"機器１８",2741,"18軸機器１８位置決完了",18,"機器１８",3541,"18軸機器１８急停止指令"]
[{"$nulls":4},18,"機器１８",2742,"18軸機器１８In-position",18,"機器１８",3542,"18軸機器１８正転JOG指令"]
[{"$nulls":4},18,"機器１８",2743,"18軸機器１８指令In-position",18,"機器１８",3543,"18軸機器１８逆転JOG指令"]
[{"$nulls":4},18,"機器１８",2744,"18軸機器１８速度制御中",18,"機器１８",3544,"18軸機器１８完了信号OFF指令"]
[{"$nulls":4},18,"機器１８",2745,"18軸機器１８速度・位置Latch",18,"機器１８",3545,"18軸機器１８速度・位置切替許可"]
[{"$nulls":4},18,"機器１８",2746,"18軸機器１８零点通過",18,"機器１８",3546,"18軸機器１８位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},18,"機器１８",2747,"18軸機器１８Error検出",18,"機器１８",3547,"18軸機器１８ｴﾗｰリセット"]
[{"$nulls":4},18,"機器１８",2748,"18軸機器１８ServoError検出",18,"機器１８",3548,"18軸機器１８ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},18,"機器１８",2749,"18軸機器１８原点復帰要求",18,"機器１８",3549,"18軸機器１８始動時の停止入力無効"]
[{"$nulls":4},18,"機器１８",2750,"18軸機器１８原点復帰完了",18,"機器１８",3550,"18軸機器１８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},18,"機器１８",2751,"18軸機器１８FLS 検出",18,"機器１８",3551,"18軸機器１８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},18,"機器１８",2752,"18軸機器１８RLS 検出",18,"機器１８",3552,"18軸機器１８送り現在値更新指令"]
[{"$nulls":4},18,"機器１８",2753,"18軸機器１８STOP 検出",18,"機器１８",3553,"18軸機器１８ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},18,"機器１８",2754,"18軸機器１８DOG/CHANGE 検出",18,"機器１８",3554,"18軸機器１８ｶﾑ基準位置設定指令"]
[{"$nulls":4},18,"機器１８",2755,"18軸機器１８ServoReady",18,"機器１８",3555,"18軸機器１８ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},18,"機器１８",2756,"18軸機器１８ﾄﾙｸ制御中",18,"機器１８",3556,"18軸機器１８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},18,"機器１８",2757,"18軸機器１８ﾕｰｻﾞ使用不可",18,"機器１８",3557,"18軸機器１８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},18,"機器１８",2758,"18軸機器１８仮想ﾓｰﾄﾞ継続不可",18,"機器１８",3558,"18軸機器１８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},18,"機器１８",2759,"18軸機器１８Mｺｰﾄﾞ出力中",18,"機器１８",3559,"18軸機器１８FIN信号"]
[{"$nulls":4},19,"機器１９",2760,"19軸機器１９位置決始動完了",19,"機器１９",3560,"19軸機器１９停止指令"]
[{"$nulls":4},19,"機器１９",2761,"19軸機器１９位置決完了",19,"機器１９",3561,"19軸機器１９急停止指令"]
[{"$nulls":4},19,"機器１９",2762,"19軸機器１９In-position",19,"機器１９",3562,"19軸機器１９正転JOG指令"]
[{"$nulls":4},19,"機器１９",2763,"19軸機器１９指令In-position",19,"機器１９",3563,"19軸機器１９逆転JOG指令"]
[{"$nulls":4},19,"機器１９",2764,"19軸機器１９速度制御中",19,"機器１９",3564,"19軸機器１９完了信号OFF指令"]
[{"$nulls":4},19,"機器１９",2765,"19軸機器１９速度・位置Latch",19,"機器１９",3565,"19軸機器１９速度・位置切替許可"]
[{"$nulls":4},19,"機器１９",2766,"19軸機器１９零点通過",19,"機器１９",3566,"19軸機器１９位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},19,"機器１９",2767,"19軸機器１９Error検出",19,"機器１９",3567,"19軸機器１９ｴﾗｰリセット"]
[{"$nulls":4},19,"機器１９",2768,"19軸機器１９ServoError検出",19,"機器１９",3568,"19軸機器１９ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},19,"機器１９",2769,"19軸機器１９原点復帰要求",19,"機器１９",3569,"19軸機器１９始動時の停止入力無効"]
[{"$nulls":4},19,"機器１９",2770,"19軸機器１９原点復帰完了",19,"機器１９",3570,"19軸機器１９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},19,"機器１９",2771,"19軸機器１９FLS 検出",19,"機器１９",3571,"19軸機器１９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},19,"機器１９",2772,"19軸機器１９RLS 検出",19,"機器１９",3572,"19軸機器１９送り現在値更新指令"]
[{"$nulls":4},19,"機器１９",2773,"19軸機器１９STOP 検出",19,"機器１９",3573,"19軸機器１９ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},19,"機器１９",2774,"19軸機器１９DOG/CHANGE 検出",19,"機器１９",3574,"19軸機器１９ｶﾑ基準位置設定指令"]
[{"$nulls":4},19,"機器１９",2775,"19軸機器１９ServoReady",19,"機器１９",3575,"19軸機器１９ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},19,"機器１９",2776,"19軸機器１９ﾄﾙｸ制御中",19,"機器１９",3576,"19軸機器１９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},19,"機器１９",2777,"19軸機器１９ﾕｰｻﾞ使用不可",19,"機器１９",3577,"19軸機器１９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},19,"機器１９",2778,"19軸機器１９仮想ﾓｰﾄﾞ継続不可",19,"機器１９",3578,"19軸機器１９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},19,"機器１９",2779,"19軸機器１９Mｺｰﾄﾞ出力中",19,"機器１９",3579,"19軸機器１９FIN信号"]
[{"$nulls":4},20,"機器２０",2780,"20軸機器２０位置決始動完了",20,"機器２０",3580,"20軸機器２０停止指令"]
[{"$nulls":4},20,"機器２０",2781,"20軸機器２０位置決完了",20,"機器２０",3581,"20軸機器２０急停止指令"]
[{"$nulls":4},20,"機器２０",2782,"20軸機器２０In-position",20,"機器２０",3582,"20軸機器２０正転JOG指令"]
[{"$nulls":4},20,"機器２０",2783,"20軸機器２０指令In-position",20,"機器２０",3583,"20軸機器２０逆転JOG指令"]
[{"$nulls":4},20,"機器２０",2784,"20軸機器２０速度制御中",20,"機器２０",3584,"20軸機器２０完了信号OFF指令"]
[{"$nulls":4},20,"機器２０",2785,"20軸機器２０速度・位置Latch",20,"機器２０",3585,"20軸機器２０速度・位置切替許可"]
[{"$nulls":4},20,"機器２０",2786,"20軸機器２０零点通過",20,"機器２０",3586,"20軸機器２０位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},20,"機器２０",2787,"20軸機器２０Error検出",20,"機器２０",3587,"20軸機器２０ｴﾗｰリセット"]
[{"$nulls":4},20,"機器２０",2788,"20軸機器２０ServoError検出",20,"機器２０",3588,"20軸機器２０ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},20,"機器２０",2789,"20軸機器２０原点復帰要求",20,"機器２０",3589,"20軸機器２０始動時の停止入力無効"]
[{"$nulls":4},20,"機器２０",2790,"20軸機器２０原点復帰完了",20,"機器２０",3590,"20軸機器２０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},20,"機器２０",2791,"20軸機器２０FLS 検出",20,"機器２０",3591,"20軸機器２０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},20,"機器２０",2792,"20軸機器２０RLS 検出",20,"機器２０",3592,"20軸機器２０送り現在値更新指令"]
[{"$nulls":4},20,"機器２０",2793,"20軸機器２０STOP 検出",20,"機器２０",3593,"20軸機器２０ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},20,"機器２０",2794,"20軸機器２０DOG/CHANGE 検出",20,"機器２０",3594,"20軸機器２０ｶﾑ基準位置設定指令"]
[{"$nulls":4},20,"機器２０",2795,"20軸機器２０ServoReady",20,"機器２０",3595,"20軸機器２０ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},20,"機器２０",2796,"20軸機器２０ﾄﾙｸ制御中",20,"機器２０",3596,"20軸機器２０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},20,"機器２０",2797,"20軸機器２０ﾕｰｻﾞ使用不可",20,"機器２０",3597,"20軸機器２０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},20,"機器２０",2798,"20軸機器２０仮想ﾓｰﾄﾞ継続不可",20,"機器２０",3598,"20軸機器２０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},20,"機器２０",2799,"20軸機器２０Mｺｰﾄﾞ出力中",20,"機器２０",3599,"20軸機器２０FIN信号"]
[{"$nulls":4},21,"機器２１",2800,"21軸機器２１位置決始動完了",21,"機器２１",3600,"21軸機器２１停止指令"]
[{"$nulls":4},21,"機器２１",2801,"21軸機器２１位置決完了",21,"機器２１",3601,"21軸機器２１急停止指令"]
[{"$nulls":4},21,"機器２１",2802,"21軸機器２１In-position",21,"機器２１",3602,"21軸機器２１正転JOG指令"]
[{"$nulls":4},21,"機器２１",2803,"21軸機器２１指令In-position",21,"機器２１",3603,"21軸機器２１逆転JOG指令"]
[{"$nulls":4},21,"機器２１",2804,"21軸機器２１速度制御中",21,"機器２１",3604,"21軸機器２１完了信号OFF指令"]
[{"$nulls":4},21,"機器２１",2805,"21軸機器２１速度・位置Latch",21,"機器２１",3605,"21軸機器２１速度・位置切替許可"]
[{"$nulls":4},21,"機器２１",2806,"21軸機器２１零点通過",21,"機器２１",3606,"21軸機器２１位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},21,"機器２１",2807,"21軸機器２１Error検出",21,"機器２１",3607,"21軸機器２１ｴﾗｰリセット"]
[{"$nulls":4},21,"機器２１",2808,"21軸機器２１ServoError検出",21,"機器２１",3608,"21軸機器２１ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},21,"機器２１",2809,"21軸機器２１原点復帰要求",21,"機器２１",3609,"21軸機器２１始動時の停止入力無効"]
[{"$nulls":4},21,"機器２１",2810,"21軸機器２１原点復帰完了",21,"機器２１",3610,"21軸機器２１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},21,"機器２１",2811,"21軸機器２１FLS 検出",21,"機器２１",3611,"21軸機器２１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},21,"機器２１",2812,"21軸機器２１RLS 検出",21,"機器２１",3612,"21軸機器２１送り現在値更新指令"]
[{"$nulls":4},21,"機器２１",2813,"21軸機器２１STOP 検出",21,"機器２１",3613,"21軸機器２１ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},21,"機器２１",2814,"21軸機器２１DOG/CHANGE 検出",21,"機器２１",3614,"21軸機器２１ｶﾑ基準位置設定指令"]
[{"$nulls":4},21,"機器２１",2815,"21軸機器２１ServoReady",21,"機器２１",3615,"21軸機器２１ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},21,"機器２１",2816,"21軸機器２１ﾄﾙｸ制御中",21,"機器２１",3616,"21軸機器２１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},21,"機器２１",2817,"21軸機器２１ﾕｰｻﾞ使用不可",21,"機器２１",3617,"21軸機器２１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},21,"機器２１",2818,"21軸機器２１仮想ﾓｰﾄﾞ継続不可",21,"機器２１",3618,"21軸機器２１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},21,"機器２１",2819,"21軸機器２１Mｺｰﾄﾞ出力中",21,"機器２１",3619,"21軸機器２１FIN信号"]
[{"$nulls":4},22,"機器２２",2820,"22軸機器２２位置決始動完了",22,"機器２２",3620,"22軸機器２２停止指令"]
[{"$nulls":4},22,"機器２２",2821,"22軸機器２２位置決完了",22,"機器２２",3621,"22軸機器２２急停止指令"]
[{"$nulls":4},22,"機器２２",2822,"22軸機器２２In-position",22,"機器２２",3622,"22軸機器２２正転JOG指令"]
[{"$nulls":4},22,"機器２２",2823,"22軸機器２２指令In-position",22,"機器２２",3623,"22軸機器２２逆転JOG指令"]
[{"$nulls":4},22,"機器２２",2824,"22軸機器２２速度制御中",22,"機器２２",3624,"22軸機器２２完了信号OFF指令"]
[{"$nulls":4},22,"機器２２",2825,"22軸機器２２速度・位置Latch",22,"機器２２",3625,"22軸機器２２速度・位置切替許可"]
[{"$nulls":4},22,"機器２２",2826,"22軸機器２２零点通過",22,"機器２２",3626,"22軸機器２２位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},22,"機器２２",2827,"22軸機器２２Error検出",22,"機器２２",3627,"22軸機器２２ｴﾗｰリセット"]
[{"$nulls":4},22,"機器２２",2828,"22軸機器２２ServoError検出",22,"機器２２",3628,"22軸機器２２ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},22,"機器２２",2829,"22軸機器２２原点復帰要求",22,"機器２２",3629,"22軸機器２２始動時の停止入力無効"]
[{"$nulls":4},22,"機器２２",2830,"22軸機器２２原点復帰完了",22,"機器２２",3630,"22軸機器２２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},22,"機器２２",2831,"22軸機器２２FLS 検出",22,"機器２２",3631,"22軸機器２２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},22,"機器２２",2832,"22軸機器２２RLS 検出",22,"機器２２",3632,"22軸機器２２送り現在値更新指令"]
[{"$nulls":4},22,"機器２２",2833,"22軸機器２２STOP 検出",22,"機器２２",3633,"22軸機器２２ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},22,"機器２２",2834,"22軸機器２２DOG/CHANGE 検出",22,"機器２２",3634,"22軸機器２２ｶﾑ基準位置設定指令"]
[{"$nulls":4},22,"機器２２",2835,"22軸機器２２ServoReady",22,"機器２２",3635,"22軸機器２２ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},22,"機器２２",2836,"22軸機器２２ﾄﾙｸ制御中",22,"機器２２",3636,"22軸機器２２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},22,"機器２２",2837,"22軸機器２２ﾕｰｻﾞ使用不可",22,"機器２２",3637,"22軸機器２２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},22,"機器２２",2838,"22軸機器２２仮想ﾓｰﾄﾞ継続不可",22,"機器２２",3638,"22軸機器２２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},22,"機器２２",2839,"22軸機器２２Mｺｰﾄﾞ出力中",22,"機器２２",3639,"22軸機器２２FIN信号"]
[{"$nulls":4},23,"機器２３",2840,"23軸機器２３位置決始動完了",23,"機器２３",3640,"23軸機器２３停止指令"]
[{"$nulls":4},23,"機器２３",2841,"23軸機器２３位置決完了",23,"機器２３",3641,"23軸機器２３急停止指令"]
[{"$nulls":4},23,"機器２３",2842,"23軸機器２３In-position",23,"機器２３",3642,"23軸機器２３正転JOG指令"]
[{"$nulls":4},23,"機器２３",2843,"23軸機器２３指令In-position",23,"機器２３",3643,"23軸機器２３逆転JOG指令"]
[{"$nulls":4},23,"機器２３",2844,"23軸機器２３速度制御中",23,"機器２３",3644,"23軸機器２３完了信号OFF指令"]
[{"$nulls":4},23,"機器２３",2845,"23軸機器２３速度・位置Latch",23,"機器２３",3645,"23軸機器２３速度・位置切替許可"]
[{"$nulls":4},23,"機器２３",2846,"23軸機器２３零点通過",23,"機器２３",3646,"23軸機器２３位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},23,"機器２３",2847,"23軸機器２３Error検出",23,"機器２３",3647,"23軸機器２３ｴﾗｰリセット"]
[{"$nulls":4},23,"機器２３",2848,"23軸機器２３ServoError検出",23,"機器２３",3648,"23軸機器２３ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},23,"機器２３",2849,"23軸機器２３原点復帰要求",23,"機器２３",3649,"23軸機器２３始動時の停止入力無効"]
[{"$nulls":4},23,"機器２３",2850,"23軸機器２３原点復帰完了",23,"機器２３",3650,"23軸機器２３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},23,"機器２３",2851,"23軸機器２３FLS 検出",23,"機器２３",3651,"23軸機器２３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},23,"機器２３",2852,"23軸機器２３RLS 検出",23,"機器２３",3652,"23軸機器２３送り現在値更新指令"]
[{"$nulls":4},23,"機器２３",2853,"23軸機器２３STOP 検出",23,"機器２３",3653,"23軸機器２３ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},23,"機器２３",2854,"23軸機器２３DOG/CHANGE 検出",23,"機器２３",3654,"23軸機器２３ｶﾑ基準位置設定指令"]
[{"$nulls":4},23,"機器２３",2855,"23軸機器２３ServoReady",23,"機器２３",3655,"23軸機器２３ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},23,"機器２３",2856,"23軸機器２３ﾄﾙｸ制御中",23,"機器２３",3656,"23軸機器２３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},23,"機器２３",2857,"23軸機器２３ﾕｰｻﾞ使用不可",23,"機器２３",3657,"23軸機器２３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},23,"機器２３",2858,"23軸機器２３仮想ﾓｰﾄﾞ継続不可",23,"機器２３",3658,"23軸機器２３ﾕｰｻﾞ使用不可"]
[{"$nulls":4},23,"機器２３",2859,"23軸機器２３Mｺｰﾄﾞ出力中",23,"機器２３",3659,"23軸機器２３FIN信号"]
[{"$nulls":4},24,"機器２４",2860,"24軸機器２４位置決始動完了",24,"機器２４",3660,"24軸機器２４停止指令"]
[{"$nulls":4},24,"機器２４",2861,"24軸機器２４位置決完了",24,"機器２４",3661,"24軸機器２４急停止指令"]
[{"$nulls":4},24,"機器２４",2862,"24軸機器２４In-position",24,"機器２４",3662,"24軸機器２４正転JOG指令"]
[{"$nulls":4},24,"機器２４",2863,"24軸機器２４指令In-position",24,"機器２４",3663,"24軸機器２４逆転JOG指令"]
[{"$nulls":4},24,"機器２４",2864,"24軸機器２４速度制御中",24,"機器２４",3664,"24軸機器２４完了信号OFF指令"]
[{"$nulls":4},24,"機器２４",2865,"24軸機器２４速度・位置Latch",24,"機器２４",3665,"24軸機器２４速度・位置切替許可"]
[{"$nulls":4},24,"機器２４",2866,"24軸機器２４零点通過",24,"機器２４",3666,"24軸機器２４位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},24,"機器２４",2867,"24軸機器２４Error検出",24,"機器２４",3667,"24軸機器２４ｴﾗｰリセット"]
[{"$nulls":4},24,"機器２４",2868,"24軸機器２４ServoError検出",24,"機器２４",3668,"24軸機器２４ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},24,"機器２４",2869,"24軸機器２４原点復帰要求",24,"機器２４",3669,"24軸機器２４始動時の停止入力無効"]
[{"$nulls":4},24,"機器２４",2870,"24軸機器２４原点復帰完了",24,"機器２４",3670,"24軸機器２４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},24,"機器２４",2871,"24軸機器２４FLS 検出",24,"機器２４",3671,"24軸機器２４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},24,"機器２４",2872,"24軸機器２４RLS 検出",24,"機器２４",3672,"24軸機器２４送り現在値更新指令"]
[{"$nulls":4},24,"機器２４",2873,"24軸機器２４STOP 検出",24,"機器２４",3673,"24軸機器２４ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},24,"機器２４",2874,"24軸機器２４DOG/CHANGE 検出",24,"機器２４",3674,"24軸機器２４ｶﾑ基準位置設定指令"]
[{"$nulls":4},24,"機器２４",2875,"24軸機器２４ServoReady",24,"機器２４",3675,"24軸機器２４ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},24,"機器２４",2876,"24軸機器２４ﾄﾙｸ制御中",24,"機器２４",3676,"24軸機器２４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},24,"機器２４",2877,"24軸機器２４ﾕｰｻﾞ使用不可",24,"機器２４",3677,"24軸機器２４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},24,"機器２４",2878,"24軸機器２４仮想ﾓｰﾄﾞ継続不可",24,"機器２４",3678,"24軸機器２４ﾕｰｻﾞ使用不可"]
[{"$nulls":4},24,"機器２４",2879,"24軸機器２４Mｺｰﾄﾞ出力中",24,"機器２４",3679,"24軸機器２４FIN信号"]
[{"$nulls":4},25,"機器２５",2880,"25軸機器２５位置決始動完了",25,"機器２５",3680,"25軸機器２５停止指令"]
[{"$nulls":4},25,"機器２５",2881,"25軸機器２５位置決完了",25,"機器２５",3681,"25軸機器２５急停止指令"]
[{"$nulls":4},25,"機器２５",2882,"25軸機器２５In-position",25,"機器２５",3682,"25軸機器２５正転JOG指令"]
[{"$nulls":4},25,"機器２５",2883,"25軸機器２５指令In-position",25,"機器２５",3683,"25軸機器２５逆転JOG指令"]
[{"$nulls":4},25,"機器２５",2884,"25軸機器２５速度制御中",25,"機器２５",3684,"25軸機器２５完了信号OFF指令"]
[{"$nulls":4},25,"機器２５",2885,"25軸機器２５速度・位置Latch",25,"機器２５",3685,"25軸機器２５速度・位置切替許可"]
[{"$nulls":4},25,"機器２５",2886,"25軸機器２５零点通過",25,"機器２５",3686,"25軸機器２５位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},25,"機器２５",2887,"25軸機器２５Error検出",25,"機器２５",3687,"25軸機器２５ｴﾗｰリセット"]
[{"$nulls":4},25,"機器２５",2888,"25軸機器２５ServoError検出",25,"機器２５",3688,"25軸機器２５ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},25,"機器２５",2889,"25軸機器２５原点復帰要求",25,"機器２５",3689,"25軸機器２５始動時の停止入力無効"]
[{"$nulls":4},25,"機器２５",2890,"25軸機器２５原点復帰完了",25,"機器２５",3690,"25軸機器２５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},25,"機器２５",2891,"25軸機器２５FLS 検出",25,"機器２５",3691,"25軸機器２５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},25,"機器２５",2892,"25軸機器２５RLS 検出",25,"機器２５",3692,"25軸機器２５送り現在値更新指令"]
[{"$nulls":4},25,"機器２５",2893,"25軸機器２５STOP 検出",25,"機器２５",3693,"25軸機器２５ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},25,"機器２５",2894,"25軸機器２５DOG/CHANGE 検出",25,"機器２５",3694,"25軸機器２５ｶﾑ基準位置設定指令"]
[{"$nulls":4},25,"機器２５",2895,"25軸機器２５ServoReady",25,"機器２５",3695,"25軸機器２５ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},25,"機器２５",2896,"25軸機器２５ﾄﾙｸ制御中",25,"機器２５",3696,"25軸機器２５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},25,"機器２５",2897,"25軸機器２５ﾕｰｻﾞ使用不可",25,"機器２５",3697,"25軸機器２５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},25,"機器２５",2898,"25軸機器２５仮想ﾓｰﾄﾞ継続不可",25,"機器２５",3698,"25軸機器２５ﾕｰｻﾞ使用不可"]
[{"$nulls":4},25,"機器２５",2899,"25軸機器２５Mｺｰﾄﾞ出力中",25,"機器２５",3699,"25軸機器２５FIN信号"]
[{"$nulls":4},26,"機器２６",2900,"26軸機器２６位置決始動完了",26,"機器２６",3700,"26軸機器２６停止指令"]
[{"$nulls":4},26,"機器２６",2901,"26軸機器２６位置決完了",26,"機器２６",3701,"26軸機器２６急停止指令"]
[{"$nulls":4},26,"機器２６",2902,"26軸機器２６In-position",26,"機器２６",3702,"26軸機器２６正転JOG指令"]
[{"$nulls":4},26,"機器２６",2903,"26軸機器２６指令In-position",26,"機器２６",3703,"26軸機器２６逆転JOG指令"]
[{"$nulls":4},26,"機器２６",2904,"26軸機器２６速度制御中",26,"機器２６",3704,"26軸機器２６完了信号OFF指令"]
[{"$nulls":4},26,"機器２６",2905,"26軸機器２６速度・位置Latch",26,"機器２６",3705,"26軸機器２６速度・位置切替許可"]
[{"$nulls":4},26,"機器２６",2906,"26軸機器２６零点通過",26,"機器２６",3706,"26軸機器２６位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},26,"機器２６",2907,"26軸機器２６Error検出",26,"機器２６",3707,"26軸機器２６ｴﾗｰリセット"]
[{"$nulls":4},26,"機器２６",2908,"26軸機器２６ServoError検出",26,"機器２６",3708,"26軸機器２６ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},26,"機器２６",2909,"26軸機器２６原点復帰要求",26,"機器２６",3709,"26軸機器２６始動時の停止入力無効"]
[{"$nulls":4},26,"機器２６",2910,"26軸機器２６原点復帰完了",26,"機器２６",3710,"26軸機器２６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},26,"機器２６",2911,"26軸機器２６FLS 検出",26,"機器２６",3711,"26軸機器２６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},26,"機器２６",2912,"26軸機器２６RLS 検出",26,"機器２６",3712,"26軸機器２６送り現在値更新指令"]
[{"$nulls":4},26,"機器２６",2913,"26軸機器２６STOP 検出",26,"機器２６",3713,"26軸機器２６ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},26,"機器２６",2914,"26軸機器２６DOG/CHANGE 検出",26,"機器２６",3714,"26軸機器２６ｶﾑ基準位置設定指令"]
[{"$nulls":4},26,"機器２６",2915,"26軸機器２６ServoReady",26,"機器２６",3715,"26軸機器２６ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},26,"機器２６",2916,"26軸機器２６ﾄﾙｸ制御中",26,"機器２６",3716,"26軸機器２６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},26,"機器２６",2917,"26軸機器２６ﾕｰｻﾞ使用不可",26,"機器２６",3717,"26軸機器２６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},26,"機器２６",2918,"26軸機器２６仮想ﾓｰﾄﾞ継続不可",26,"機器２６",3718,"26軸機器２６ﾕｰｻﾞ使用不可"]
[{"$nulls":4},26,"機器２６",2919,"26軸機器２６Mｺｰﾄﾞ出力中",26,"機器２６",3719,"26軸機器２６FIN信号"]
[{"$nulls":4},27,"機器２７",2920,"27軸機器２７位置決始動完了",27,"機器２７",3720,"27軸機器２７停止指令"]
[{"$nulls":4},27,"機器２７",2921,"27軸機器２７位置決完了",27,"機器２７",3721,"27軸機器２７急停止指令"]
[{"$nulls":4},27,"機器２７",2922,"27軸機器２７In-position",27,"機器２７",3722,"27軸機器２７正転JOG指令"]
[{"$nulls":4},27,"機器２７",2923,"27軸機器２７指令In-position",27,"機器２７",3723,"27軸機器２７逆転JOG指令"]
[{"$nulls":4},27,"機器２７",2924,"27軸機器２７速度制御中",27,"機器２７",3724,"27軸機器２７完了信号OFF指令"]
[{"$nulls":4},27,"機器２７",2925,"27軸機器２７速度・位置Latch",27,"機器２７",3725,"27軸機器２７速度・位置切替許可"]
[{"$nulls":4},27,"機器２７",2926,"27軸機器２７零点通過",27,"機器２７",3726,"27軸機器２７位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},27,"機器２７",2927,"27軸機器２７Error検出",27,"機器２７",3727,"27軸機器２７ｴﾗｰリセット"]
[{"$nulls":4},27,"機器２７",2928,"27軸機器２７ServoError検出",27,"機器２７",3728,"27軸機器２７ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},27,"機器２７",2929,"27軸機器２７原点復帰要求",27,"機器２７",3729,"27軸機器２７始動時の停止入力無効"]
[{"$nulls":4},27,"機器２７",2930,"27軸機器２７原点復帰完了",27,"機器２７",3730,"27軸機器２７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},27,"機器２７",2931,"27軸機器２７FLS 検出",27,"機器２７",3731,"27軸機器２７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},27,"機器２７",2932,"27軸機器２７RLS 検出",27,"機器２７",3732,"27軸機器２７送り現在値更新指令"]
[{"$nulls":4},27,"機器２７",2933,"27軸機器２７STOP 検出",27,"機器２７",3733,"27軸機器２７ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},27,"機器２７",2934,"27軸機器２７DOG/CHANGE 検出",27,"機器２７",3734,"27軸機器２７ｶﾑ基準位置設定指令"]
[{"$nulls":4},27,"機器２７",2935,"27軸機器２７ServoReady",27,"機器２７",3735,"27軸機器２７ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},27,"機器２７",2936,"27軸機器２７ﾄﾙｸ制御中",27,"機器２７",3736,"27軸機器２７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},27,"機器２７",2937,"27軸機器２７ﾕｰｻﾞ使用不可",27,"機器２７",3737,"27軸機器２７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},27,"機器２７",2938,"27軸機器２７仮想ﾓｰﾄﾞ継続不可",27,"機器２７",3738,"27軸機器２７ﾕｰｻﾞ使用不可"]
[{"$nulls":4},27,"機器２７",2939,"27軸機器２７Mｺｰﾄﾞ出力中",27,"機器２７",3739,"27軸機器２７FIN信号"]
[{"$nulls":4},28,"機器２８",2940,"28軸機器２８位置決始動完了",28,"機器２８",3740,"28軸機器２８停止指令"]
[{"$nulls":4},28,"機器２８",2941,"28軸機器２８位置決完了",28,"機器２８",3741,"28軸機器２８急停止指令"]
[{"$nulls":4},28,"機器２８",2942,"28軸機器２８In-position",28,"機器２８",3742,"28軸機器２８正転JOG指令"]
[{"$nulls":4},28,"機器２８",2943,"28軸機器２８指令In-position",28,"機器２８",3743,"28軸機器２８逆転JOG指令"]
[{"$nulls":4},28,"機器２８",2944,"28軸機器２８速度制御中",28,"機器２８",3744,"28軸機器２８完了信号OFF指令"]
[{"$nulls":4},28,"機器２８",2945,"28軸機器２８速度・位置Latch",28,"機器２８",3745,"28軸機器２８速度・位置切替許可"]
[{"$nulls":4},28,"機器２８",2946,"28軸機器２８零点通過",28,"機器２８",3746,"28軸機器２８位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},28,"機器２８",2947,"28軸機器２８Error検出",28,"機器２８",3747,"28軸機器２８ｴﾗｰリセット"]
[{"$nulls":4},28,"機器２８",2948,"28軸機器２８ServoError検出",28,"機器２８",3748,"28軸機器２８ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},28,"機器２８",2949,"28軸機器２８原点復帰要求",28,"機器２８",3749,"28軸機器２８始動時の停止入力無効"]
[{"$nulls":4},28,"機器２８",2950,"28軸機器２８原点復帰完了",28,"機器２８",3750,"28軸機器２８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},28,"機器２８",2951,"28軸機器２８FLS 検出",28,"機器２８",3751,"28軸機器２８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},28,"機器２８",2952,"28軸機器２８RLS 検出",28,"機器２８",3752,"28軸機器２８送り現在値更新指令"]
[{"$nulls":4},28,"機器２８",2953,"28軸機器２８STOP 検出",28,"機器２８",3753,"28軸機器２８ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},28,"機器２８",2954,"28軸機器２８DOG/CHANGE 検出",28,"機器２８",3754,"28軸機器２８ｶﾑ基準位置設定指令"]
[{"$nulls":4},28,"機器２８",2955,"28軸機器２８ServoReady",28,"機器２８",3755,"28軸機器２８ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},28,"機器２８",2956,"28軸機器２８ﾄﾙｸ制御中",28,"機器２８",3756,"28軸機器２８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},28,"機器２８",2957,"28軸機器２８ﾕｰｻﾞ使用不可",28,"機器２８",3757,"28軸機器２８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},28,"機器２８",2958,"28軸機器２８仮想ﾓｰﾄﾞ継続不可",28,"機器２８",3758,"28軸機器２８ﾕｰｻﾞ使用不可"]
[{"$nulls":4},28,"機器２８",2959,"28軸機器２８Mｺｰﾄﾞ出力中",28,"機器２８",3759,"28軸機器２８FIN信号"]
[{"$nulls":4},29,"機器２９",2960,"29軸機器２９位置決始動完了",29,"機器２９",3760,"29軸機器２９停止指令"]
[{"$nulls":4},29,"機器２９",2961,"29軸機器２９位置決完了",29,"機器２９",3761,"29軸機器２９急停止指令"]
[{"$nulls":4},29,"機器２９",2962,"29軸機器２９In-position",29,"機器２９",3762,"29軸機器２９正転JOG指令"]
[{"$nulls":4},29,"機器２９",2963,"29軸機器２９指令In-position",29,"機器２９",3763,"29軸機器２９逆転JOG指令"]
[{"$nulls":4},29,"機器２９",2964,"29軸機器２９速度制御中",29,"機器２９",3764,"29軸機器２９完了信号OFF指令"]
[{"$nulls":4},29,"機器２９",2965,"29軸機器２９速度・位置Latch",29,"機器２９",3765,"29軸機器２９速度・位置切替許可"]
[{"$nulls":4},29,"機器２９",2966,"29軸機器２９零点通過",29,"機器２９",3766,"29軸機器２９位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},29,"機器２９",2967,"29軸機器２９Error検出",29,"機器２９",3767,"29軸機器２９ｴﾗｰリセット"]
[{"$nulls":4},29,"機器２９",2968,"29軸機器２９ServoError検出",29,"機器２９",3768,"29軸機器２９ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},29,"機器２９",2969,"29軸機器２９原点復帰要求",29,"機器２９",3769,"29軸機器２９始動時の停止入力無効"]
[{"$nulls":4},29,"機器２９",2970,"29軸機器２９原点復帰完了",29,"機器２９",3770,"29軸機器２９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},29,"機器２９",2971,"29軸機器２９FLS 検出",29,"機器２９",3771,"29軸機器２９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},29,"機器２９",2972,"29軸機器２９RLS 検出",29,"機器２９",3772,"29軸機器２９送り現在値更新指令"]
[{"$nulls":4},29,"機器２９",2973,"29軸機器２９STOP 検出",29,"機器２９",3773,"29軸機器２９ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},29,"機器２９",2974,"29軸機器２９DOG/CHANGE 検出",29,"機器２９",3774,"29軸機器２９ｶﾑ基準位置設定指令"]
[{"$nulls":4},29,"機器２９",2975,"29軸機器２９ServoReady",29,"機器２９",3775,"29軸機器２９ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},29,"機器２９",2976,"29軸機器２９ﾄﾙｸ制御中",29,"機器２９",3776,"29軸機器２９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},29,"機器２９",2977,"29軸機器２９ﾕｰｻﾞ使用不可",29,"機器２９",3777,"29軸機器２９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},29,"機器２９",2978,"29軸機器２９仮想ﾓｰﾄﾞ継続不可",29,"機器２９",3778,"29軸機器２９ﾕｰｻﾞ使用不可"]
[{"$nulls":4},29,"機器２９",2979,"29軸機器２９Mｺｰﾄﾞ出力中",29,"機器２９",3779,"29軸機器２９FIN信号"]
[{"$nulls":4},30,"機器３０",2980,"30軸機器３０位置決始動完了",30,"機器３０",3780,"30軸機器３０停止指令"]
[{"$nulls":4},30,"機器３０",2981,"30軸機器３０位置決完了",30,"機器３０",3781,"30軸機器３０急停止指令"]
[{"$nulls":4},30,"機器３０",2982,"30軸機器３０In-position",30,"機器３０",3782,"30軸機器３０正転JOG指令"]
[{"$nulls":4},30,"機器３０",2983,"30軸機器３０指令In-position",30,"機器３０",3783,"30軸機器３０逆転JOG指令"]
[{"$nulls":4},30,"機器３０",2984,"30軸機器３０速度制御中",30,"機器３０",3784,"30軸機器３０完了信号OFF指令"]
[{"$nulls":4},30,"機器３０",2985,"30軸機器３０速度・位置Latch",30,"機器３０",3785,"30軸機器３０速度・位置切替許可"]
[{"$nulls":4},30,"機器３０",2986,"30軸機器３０零点通過",30,"機器３０",3786,"30軸機器３０位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},30,"機器３０",2987,"30軸機器３０Error検出",30,"機器３０",3787,"30軸機器３０ｴﾗｰリセット"]
[{"$nulls":4},30,"機器３０",2988,"30軸機器３０ServoError検出",30,"機器３０",3788,"30軸機器３０ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},30,"機器３０",2989,"30軸機器３０原点復帰要求",30,"機器３０",3789,"30軸機器３０始動時の停止入力無効"]
[{"$nulls":4},30,"機器３０",2990,"30軸機器３０原点復帰完了",30,"機器３０",3790,"30軸機器３０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},30,"機器３０",2991,"30軸機器３０FLS 検出",30,"機器３０",3791,"30軸機器３０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},30,"機器３０",2992,"30軸機器３０RLS 検出",30,"機器３０",3792,"30軸機器３０送り現在値更新指令"]
[{"$nulls":4},30,"機器３０",2993,"30軸機器３０STOP 検出",30,"機器３０",3793,"30軸機器３０ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},30,"機器３０",2994,"30軸機器３０DOG/CHANGE 検出",30,"機器３０",3794,"30軸機器３０ｶﾑ基準位置設定指令"]
[{"$nulls":4},30,"機器３０",2995,"30軸機器３０ServoReady",30,"機器３０",3795,"30軸機器３０ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},30,"機器３０",2996,"30軸機器３０ﾄﾙｸ制御中",30,"機器３０",3796,"30軸機器３０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},30,"機器３０",2997,"30軸機器３０ﾕｰｻﾞ使用不可",30,"機器３０",3797,"30軸機器３０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},30,"機器３０",2998,"30軸機器３０仮想ﾓｰﾄﾞ継続不可",30,"機器３０",3798,"30軸機器３０ﾕｰｻﾞ使用不可"]
[{"$nulls":4},30,"機器３０",2999,"30軸機器３０Mｺｰﾄﾞ出力中",30,"機器３０",3799,"30軸機器３０FIN信号"]
[{"$nulls":4},31,"機器３１",3000,"31軸機器３１位置決始動完了",31,"機器３１",3800,"31軸機器３１停止指令"]
[{"$nulls":4},31,"機器３１",3001,"31軸機器３１位置決完了",31,"機器３１",3801,"31軸機器３１急停止指令"]
[{"$nulls":4},31,"機器３１",3002,"31軸機器３１In-position",31,"機器３１",3802,"31軸機器３１正転JOG指令"]
[{"$nulls":4},31,"機器３１",3003,"31軸機器３１指令In-position",31,"機器３１",3803,"31軸機器３１逆転JOG指令"]
[{"$nulls":4},31,"機器３１",3004,"31軸機器３１速度制御中",31,"機器３１",3804,"31軸機器３１完了信号OFF指令"]
[{"$nulls":4},31,"機器３１",3005,"31軸機器３１速度・位置Latch",31,"機器３１",3805,"31軸機器３１速度・位置切替許可"]
[{"$nulls":4},31,"機器３１",3006,"31軸機器３１零点通過",31,"機器３１",3806,"31軸機器３１位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},31,"機器３１",3007,"31軸機器３１Error検出",31,"機器３１",3807,"31軸機器３１ｴﾗｰリセット"]
[{"$nulls":4},31,"機器３１",3008,"31軸機器３１ServoError検出",31,"機器３１",3808,"31軸機器３１ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},31,"機器３１",3009,"31軸機器３１原点復帰要求",31,"機器３１",3809,"31軸機器３１始動時の停止入力無効"]
[{"$nulls":4},31,"機器３１",3010,"31軸機器３１原点復帰完了",31,"機器３１",3810,"31軸機器３１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},31,"機器３１",3011,"31軸機器３１FLS 検出",31,"機器３１",3811,"31軸機器３１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},31,"機器３１",3012,"31軸機器３１RLS 検出",31,"機器３１",3812,"31軸機器３１送り現在値更新指令"]
[{"$nulls":4},31,"機器３１",3013,"31軸機器３１STOP 検出",31,"機器３１",3813,"31軸機器３１ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},31,"機器３１",3014,"31軸機器３１DOG/CHANGE 検出",31,"機器３１",3814,"31軸機器３１ｶﾑ基準位置設定指令"]
[{"$nulls":4},31,"機器３１",3015,"31軸機器３１ServoReady",31,"機器３１",3815,"31軸機器３１ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},31,"機器３１",3016,"31軸機器３１ﾄﾙｸ制御中",31,"機器３１",3816,"31軸機器３１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},31,"機器３１",3017,"31軸機器３１ﾕｰｻﾞ使用不可",31,"機器３１",3817,"31軸機器３１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},31,"機器３１",3018,"31軸機器３１仮想ﾓｰﾄﾞ継続不可",31,"機器３１",3818,"31軸機器３１ﾕｰｻﾞ使用不可"]
[{"$nulls":4},31,"機器３１",3019,"31軸機器３１Mｺｰﾄﾞ出力中",31,"機器３１",3819,"31軸機器３１FIN信号"]
[{"$nulls":4},32,"機器３２",3020,"32軸機器３２位置決始動完了",32,"機器３２",3820,"32軸機器３２停止指令"]
[{"$nulls":4},32,"機器３２",3021,"32軸機器３２位置決完了",32,"機器３２",3821,"32軸機器３２急停止指令"]
[{"$nulls":4},32,"機器３２",3022,"32軸機器３２In-position",32,"機器３２",3822,"32軸機器３２正転JOG指令"]
[{"$nulls":4},32,"機器３２",3023,"32軸機器３２指令In-position",32,"機器３２",3823,"32軸機器３２逆転JOG指令"]
[{"$nulls":4},32,"機器３２",3024,"32軸機器３２速度制御中",32,"機器３２",3824,"32軸機器３２完了信号OFF指令"]
[{"$nulls":4},32,"機器３２",3025,"32軸機器３２速度・位置Latch",32,"機器３２",3825,"32軸機器３２速度・位置切替許可"]
[{"$nulls":4},32,"機器３２",3026,"32軸機器３２零点通過",32,"機器３２",3826,"32軸機器３２位置決ﾃﾞｰﾀ更新待ち"]
[{"$nulls":4},32,"機器３２",3027,"32軸機器３２Error検出",32,"機器３２",3827,"32軸機器３２ｴﾗｰリセット"]
[{"$nulls":4},32,"機器３２",3028,"32軸機器３２ServoError検出",32,"機器３２",3828,"32軸機器３２ｻｰﾎﾞｴﾗｰリセット"]
[{"$nulls":4},32,"機器３２",3029,"32軸機器３２原点復帰要求",32,"機器３２",3829,"32軸機器３２始動時の停止入力無効"]
[{"$nulls":4},32,"機器３２",3030,"32軸機器３２原点復帰完了",32,"機器３２",3830,"32軸機器３２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},32,"機器３２",3031,"32軸機器３２FLS 検出",32,"機器３２",3831,"32軸機器３２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},32,"機器３２",3032,"32軸機器３２RLS 検出",32,"機器３２",3832,"32軸機器３２送り現在値更新指令"]
[{"$nulls":4},32,"機器３２",3033,"32軸機器３２STOP 検出",32,"機器３２",3833,"32軸機器３２ｱﾄﾞﾚｽｸﾗｯﾁ基準設定指令"]
[{"$nulls":4},32,"機器３２",3034,"32軸機器３２DOG/CHANGE 検出",32,"機器３２",3834,"32軸機器３２ｶﾑ基準位置設定指令"]
[{"$nulls":4},32,"機器３２",3035,"32軸機器３２ServoReady",32,"機器３２",3835,"32軸機器３２ｻｰﾎﾞｵﾌ指令"]
[{"$nulls":4},32,"機器３２",3036,"32軸機器３２ﾄﾙｸ制御中",32,"機器３２",3836,"32軸機器３２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},32,"機器３２",3037,"32軸機器３２ﾕｰｻﾞ使用不可",32,"機器３２",3837,"32軸機器３２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},32,"機器３２",3038,"32軸機器３２仮想ﾓｰﾄﾞ継続不可",32,"機器３２",3838,"32軸機器３２ﾕｰｻﾞ使用不可"]
[{"$nulls":4},32,"機器３２",3039,"32軸機器３２Mｺｰﾄﾞ出力中",32,"機器３２",3839,"32軸機器３２FIN信号"]